{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["水电安装工程"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"水电安装工程","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,6],[1,7,1,9],[1,10,1,11],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,7],[2,8,3,8],[2,10,2,11],[4,1,4,2],[4,6,4,7],[4,9,4,10],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,1,13,2],[13,6,13,7],[14,1,14,2],[14,6,14,7],[15,1,15,2],[15,6,15,7],[15,9,15,10],[16,1,16,2],[16,6,16,7],[16,9,16,10],[17,1,17,2],[17,6,17,7],[17,9,17,10],[18,1,18,2],[18,6,18,7],[18,9,18,10],[19,1,19,2],[19,6,19,7],[19,9,19,10],[20,1,20,2],[20,6,20,7],[20,9,20,10],[21,1,21,2],[21,6,21,7],[21,9,21,10],[22,1,22,2],[22,6,22,7],[22,9,22,10],[23,1,23,2],[23,6,23,7],[23,9,23,10],[24,1,24,2],[24,6,24,7],[24,9,24,10],[25,1,25,2],[25,6,25,7],[25,9,25,10],[26,1,26,2],[26,6,26,7],[26,9,26,10],[27,1,27,2],[27,6,27,7],[27,9,27,10],[28,1,28,2],[28,6,28,7],[28,9,28,10],[29,1,29,2],[29,6,29,7],[29,9,29,10],[30,1,30,2],[30,6,30,7],[30,9,30,10],[31,1,31,2],[31,6,31,7],[31,9,31,10],[32,1,32,2],[32,6,32,7],[32,9,32,10],[33,1,33,2],[33,6,33,7],[33,9,33,10],[34,1,34,2],[34,6,34,7],[34,9,34,10],[35,1,35,2],[35,6,35,7],[35,9,35,10],[36,1,36,2],[36,6,36,7],[36,9,36,10],[37,1,37,2],[37,6,37,7],[37,9,37,10],[38,1,38,2],[38,6,38,7],[38,9,38,10],[39,1,39,2],[39,6,39,7],[39,9,39,10],[40,1,40,2],[40,6,40,7],[40,9,40,10],[41,1,41,2],[41,6,41,7],[41,9,41,10],[42,1,42,2],[42,6,42,7],[42,9,42,10],[43,1,43,2],[43,6,43,7],[43,9,43,10],[44,1,44,2],[44,6,44,7],[44,9,44,10],[45,1,45,2],[45,6,45,7],[45,9,45,10],[46,1,46,2],[46,6,46,7],[46,9,46,10],[47,1,47,2],[47,6,47,7],[47,9,47,10],[48,0,48,8],[48,9,48,11]],"flags":["formulas_cached_only"]}
["泸州航空航天产业孵化中心室外景观绿化工程水电安装工程工程量清单与报价表","","","","","","","","","","",""]
["工程名称：","","水电安装工程","","","","",null,"","","",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","全费用单价限价(元)","","金额（元）"]
["","","","","","","","",null,"合价","全费用单价","合  计"]
[" "," ","","总平电气"," "," "," ",""," "," ",""," "]
["1","040801010836","","配电箱 AW","1.名称 ：室内配电箱AW（21个回路）\r\n2.规格型号：\r\n3.安装方式：室内挂于墙上","台","1","","7438.26"]
["2","040803001837","","电缆 YJV22-5X10","1.名称 ：电力电缆\r\n2.配线形式：管内敷设\r\n3.规格型号：配线 YJV22-5X10，已在单价中考虑波形系数\r\n4.配线部位：照明线路 综合考虑\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","m","10","","44.61"]
["3","040803002838","","镀锌钢管保护管 SC50","1.名称：钢管\r\n2.材质：镀锌保护管\r\n3.规格：SC50\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.其他：满足设计及规范要求","m","10","","69.02"]
["4","030408006871","","户内干包式 铜芯电力电缆头 YJV22-5X10  终端头","1.名称：铜芯电力电缆头  YJV22-5X10 终端头","个","2","","75.69"]
["5","040804002180","","电力电缆ZS- YJV-3x4","1.名称 ：电力电缆\r\n2.配线形式：管内敷设\r\n3.规格型号：配线 ZS-YJV-3x4，已在单价中考虑波形系数\r\n4.配线部位：照明线路 综合考虑\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","m","373.064","","19.13"]
["6","040804001181","","埋地配管 PVC32","1.名称：塑料管\r\n2.材质：埋地阻燃塑料管\r\n3.规格：PVC32\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.其他：满足设计及规范要求","m","204.264","","17.03"]
["7","030408006872","","户内干包式 铜芯电力电缆头 ZS-YJV-3x4  终端头","1.名称：铜芯电力电缆头 ZS-YJV-3x4  终端头","个","8","","73.14"]
["8","040804002180","","电力电缆 ZS-YJV-3x2.5","1.名称 ：电力电缆\r\n2.配线形式：管内敷设\r\n3.规格型号：配线 ZS-YJV-3x2.5，已在单价中考虑波形系数\r\n4.配线部位：照明线路 综合考虑\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","m","265.18","","17.24"]
["9","040804001181","","埋地配管 PVC16","1.名称：塑料管\r\n2.材质：埋地阻燃塑料管\r\n3.规格：PVC16\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.其他：满足设计及规范要求","m","180.78","","10.99"]
["10","030408006872","","户内干包式 铜芯电力电缆头ZS- YJV-3x2.5  终端头","1.名称：铜芯电力电缆头 ZS-YJV-3x4  终端头","个","2","","73.14"]
["11","040804002180","","电力电缆 YJV-3x2.5","1.名称 ：电力电缆\r\n2.配线形式：管内敷设\r\n3.规格型号：配线 YJV-3x2.5已在单价中考虑波形系数\r\n4.配线部位：照明线路 综合考虑\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","m","990.523","","13.73",null,null,""]
["12","040804001181","","埋地配管 PVC16","1.名称：塑料管\r\n2.材质：埋地阻燃塑料管\r\n3.规格：PVC16\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.其他：满足设计及规范要求","m","821.723","","10.99",null,null,""]
["13","030408006872","","户内干包式 铜芯电力电缆头 YJV-3x2.5  终端头","1.名称：铜芯电力电缆头 YJV-3x2.5  终端头","个","4","","73.14",null,null,""]
["14","040804002180","","电力电缆 YJV-3x4","1.名称 ：电力电缆\r\n2.配线形式：管内敷设\r\n3.规格型号：配线 YJV-3x4，已在单价中考虑波形系数\r\n4.配线部位：照明线路 综合考虑\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","m","1764.006","","15.89",null,null,""]
["15","040804001181","","埋地配管 PVC25","1.名称：塑料管\r\n2.材质：埋地阻燃塑料管\r\n3.规格：PVC25\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.其他：满足设计及规范要求","m","1073.206","","14.55",null,null,""]
["16","030408006872","","户内干包式 铜芯电力电缆头 YJV-3x4  终端头","1.名称：铜芯电力电缆头 YJV-3x4  终端头","个","28","","73.14",null,null,""]
["17","030408006874","","户内干包式 铜芯电力电缆头 YJV-3x4  中间头","1.名称：铜芯电力电缆头 YJV-3x4  中间头","个","8","","98.05",null,null,""]
["18","040803007182","","铺砂、盖保护板（砖）一根管线","1.名称：砖保护层\r\n2.其他：满足设计及规范要求，做法详设计","m","2148.76","","10.73",null,null,""]
["19","040501004844","","车行道 线缆过路保护管  PPR DN110","1.垫层、基础材质及厚度 ：C20商品混凝土\r\n2.材质及规格 :PPR DN110\r\n3.连接形式 \r\n4.铺设深度 ：埋深1.05m，人工开挖线缆管沟，就近回填\r\n5.其他：满足设计及规范要求，做法详设计","m","100","","143.94",null,null,""]
["20","040805002847","","庭院灯","1.名称：庭院灯 40W  LED 黄光，高度不低于3.5米单杆带透光罩的庭院灯具，配光类型为半截光型，灯具样式等详见附图（灯具甲供）\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%，灯杆下杆线为  BVV-450/750V-3x2.5，综合考虑长度为4米，灯杆需提供三类防雷措施。\r\n3.垫层、基础： 150厚碎石垫层，100厚C15砼垫层，400*400 C25 钢筋砼灯柱基础，12*400*400镀锌钢板，10*400*400镀锌钢板，4套M25锚栓\r\n4.其他：满足设计及现行技术、质量、施工验收规范要求","套","33","","607.28",null,null,""]
["21","030412001848","","景观石亮化灯具","1.名称：景观石亮化灯具  40W，LED，黄光（灯具甲供）\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。\r\n3.其他：满足设计及现行技术、质量、施工验收规范要求","套","12","","41.96",null,null,""]
["22","030412001848","","建筑立面照射灯","1.名称：建筑立面照射灯  200W，LED，黄光（灯具甲供）\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。\r\n3.其他：满足设计及现行技术、质量、施工验收规范要求","套","16","","41.96",null,null,""]
["23","030412004850","","LED硬条灯","1.名称 ：LED硬条灯 18W/m  LED 黄光（灯具甲供）\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。\r\n3.位置：沿墙安装\r\n4.其他：满足设计及现行技术、质量、施工验收规范要求","套","862","","26.06",null,null,""]
["24","030412001848","","照树灯","1.名称：照树灯  100W，LED，黄光（灯具甲供）\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。\r\n3.其他：满足设计及现行技术、质量、施工验收规范要求","套","9","","41.96",null,null,""]
["25","030412002878","","球场灯","1.名称：球场灯  300W，黄光，LED（灯具甲供）\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。\r\n3.其他：满足设计及现行技术、质量、施工验收规范要求","套","8","","39.91",null,null,""]
["26","030411003879","","桥架（CT 100*50)","1.名称：金属桥架，暗敷与吊顶内\r\n2.型号：CT  100*50","m","84.4","","105.57",null,null,""]
["27","030109011880","","跌水景观加压泵 1.5KW","1.名称:跌水景观加压泵\r\n2.型号: QSP15-26-1.5","台","2","","3306.09",null,null,""]
["28","030109011880","","跌水景观加压泵 0.5KW","1.名称:跌水景观加压泵\r\n2.型号: QSP15-26-0.5","台","1","","2855.09",null,null,""]
["29","030109011880","","跌水景观循环泵 1.5KW","1.名称:跌水景观循环泵\r\n2.型号:DFE40-160A/2/1.5","台","1","","3757.09",null,null,""]
[" "," ","","给排水"," "," "," ",""," ",null,null,""]
["30","010101007001","","管沟土方","1.土壤类别 \r\n2.管外径 \r\n3.挖沟深度 \r\n4.回填要求","m3","508.077","","4.39",null,null,""]
["31","010404001862","","砂包管","1.砂包管规格详见设计图\r\n2.其他：满足设计及规范要求","m3","239.721","","217.35",null,null,""]
["32","031003001863","","DN25拔插式全铜快速取水阀","1.类型：拔插式快速取水阀，成品VB708塑料阀门箱\r\n2.材质：全铜\r\n3.规格、压力等级：DN25   200*200*200C20砼墩子\r\n4.其他：满足设计及规范要求","个","35","","331.08",null,null,""]
["33","010501006870","","C20砼镇墩  400*400*400","1.混凝土种类：给水主管  C20砼镇墩  400*400*400\r\n2.其他：做法详见设计，满足设计及规范要求","套","16","","64.38",null,null,""]
["34","040504001869","","阀门井（1000*1000*1000）","1.垫层、基础材质及厚度 ：100mmC15混凝土基础\r\n2.砌筑材料品种、规格、强度等级 ：240mm厚M7.5水泥砂浆MU10标砖\r\n3.勾缝、抹面要求 ：1：2.5水泥砂浆抹面\r\n4.盖板材质、规格 ：预制钢筋混凝土盖板，D700复合材料成品井盖\r\n5.其他：土方开挖后，就近回填，做法详见设计，满足设计及规范要求","座","6","","1258.07",null,null,""]
["35","031003001875","","全铜闸阀DN50","1.安装部位：室外 \r\n2.型号、规格 ：采用全铜闸阀DN50，阀门公称压力1.60MPa，丝口。\r\n3.其他：满足设计及规范要求","个","4","","130.68",null,null,""]
["36","031003001875","","截止阀DN25","1.安装部位：室外 \r\n2.型号、规格 ：采用全铜截止阀DN25，阀门公称压力1.60MPa，丝口。\r\n3.其他：满足设计及规范要求","个","2","","130.09",null,null,""]
["37","031001006853","","PE给水管  DN25","1.安装部位：室外\r\n2.介质：给水（冷水）\r\n3.材质、规格：PE管给水冷水管 DN25 ，PE100级聚乙烯塑料给水管，公称压力为1.6MPa。\r\n4.连接形式：热熔连接\r\n5.压力试验及吹、洗设计要求：满足设计及规范要求\r\n6.含管道支架制作、安装，带丝管件综合考虑\r\n7.其他：满足设计及规范要求","m","781.77","","20.12",null,null,""]
["38","031001006855","","PE给水管  DN40","1.安装部位：室外\r\n2.介质：给水（冷水）\r\n3.材质、规格：PE管给水冷水管 DN40，PE100级聚乙烯塑料给水管，公称压力为1.6MPa。\r\n4.连接形式：热熔连接 \r\n5.压力试验及吹、洗设计要求：满足设计及规范要求\r\n6.含管道支架制作、安装，带丝管件综合考虑\r\n7.其他：满足设计及规范要求","m","83.3","","21.50",null,null,""]
["39","031001006856","","PE给水管  DN50","1.安装部位：室外\r\n2.介质：给水（冷水）\r\n3.材质、规格：PE管给水冷水管 DN50 ，PE100级聚乙烯塑料给水管，公称压力为1.6MPa。\r\n4.连接形式：热熔连接 \r\n5.压力试验及吹、洗设计要求：满足设计及规范要求\r\n6.含管道支架制作、安装，带丝管件综合考虑\r\n7.其他：满足设计及规范要求","m","352.88","","29.77",null,null,""]
["40","031001006857","","PE给水管  DN65","1.安装部位：室外\r\n2.介质：给水（冷水）\r\n3.材质、规格：PE管给水冷水管 DN65 ，PE100级聚乙烯塑料给水管，公称压力为1.6MPa。 \r\n4.连接形式：热熔连接 \r\n5.压力试验及吹、洗设计要求：满足设计及规范要求\r\n6.含管道支架制作、安装，带丝管件综合考虑\r\n7.其他：满足设计及规范要求","m","36.84","","40.87",null,null,""]
["41","031001006858","","PE给水管  DN80","1.安装部位：室外\r\n2.介质：给水（冷水）\r\n3.材质、规格：PE管给水冷水管 DN80  ，PE100级聚乙烯塑料给水管，公称压力为1.6MPa。\r\n4.连接形式：热熔连接 \r\n5.压力试验及吹、洗设计要求：满足设计及规范要求\r\n6.含管道支架制作、安装，带丝管件综合考虑\r\n7.其他：满足设计及规范要求","m","12.86","","58.72",null,null,""]
["42","031001006881","","PVC排水管  DE110","1.安装部位：室外\r\n2.介质：排水\r\n3.材质、规格：PVC排水管  DE110。\r\n4.连接形式：粘接连接 \r\n5.压力试验及吹、洗设计要求：满足设计及规范要求\r\n6.含管道支架制作、安装，带丝管件综合考虑\r\n7.其他：满足设计及规范要求","m","100","","27.27",null,null,""]
["合　　计（大写：                                                  ）","","","","","","","","",""]