{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["【园林绿化工程】"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"【园林绿化工程】","index":0,"n_rows":91,"n_cols":11,"rows_kept":91,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,6],[1,7,1,8],[1,9,1,10],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,7],[2,8,3,8],[2,9,2,10],[4,1,4,2],[4,3,4,4],[4,6,4,7],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,3,9,4],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,1,13,2],[13,6,13,7],[14,1,14,2],[14,6,14,7],[15,1,15,2],[15,6,15,7],[16,1,16,2],[16,6,16,7],[17,1,17,2],[17,6,17,7],[18,1,18,2],[18,6,18,7],[19,1,19,2],[19,6,19,7],[20,1,20,2],[20,6,20,7],[21,1,21,2],[21,6,21,7],[22,1,22,2],[22,6,22,7],[23,1,23,2],[23,6,23,7],[24,1,24,2],[24,6,24,7],[25,1,25,2],[25,6,25,7],[26,1,26,2],[26,6,26,7],[27,1,27,2],[27,6,27,7],[28,1,28,2],[28,6,28,7],[29,1,29,2],[29,6,29,7],[30,1,30,2],[30,3,30,4],[30,6,30,7],[31,1,31,2],[31,6,31,7],[32,1,32,2],[32,6,32,7],[33,1,33,2],[33,6,33,7],[34,1,34,2],[34,6,34,7],[35,1,35,2],[35,3,35,4],[35,6,35,7],[36,1,36,2],[36,6,36,7],[37,1,37,2],[37,6,37,7],[38,1,38,2],[38,6,38,7],[39,1,39,2],[39,6,39,7],[40,1,40,2],[40,6,40,7],[41,1,41,2],[41,6,41,7],[42,1,42,2],[42,6,42,7],[43,1,43,2],[43,6,43,7],[44,1,44,2],[44,6,44,7],[45,1,45,2],[45,6,45,7],[46,1,46,2],[46,6,46,7],[47,1,47,2],[47,6,47,7],[48,1,48,2],[48,6,48,7],[49,1,49,2],[49,6,49,7],[50,1,50,2],[50,6,50,7],[51,1,51,2],[51,6,51,7],[52,1,52,2],[52,6,52,7],[53,1,53,2],[53,6,53,7],[54,1,54,2],[54,6,54,7],[55,1,55,2],[55,6,55,7],[56,1,56,2],[56,6,56,7],[57,1,57,2],[57,6,57,7],[58,1,58,2],[58,6,58,7],[59,1,59,2],[59,6,59,7],[60,1,60,2],[60,6,60,7],[61,1,61,2],[61,6,61,7],[62,1,62,2],[62,6,62,7],[63,1,63,2],[63,6,63,7],[64,1,64,2],[64,6,64,7],[65,1,65,2],[65,6,65,7],[66,1,66,2],[66,6,66,7],[67,1,67,2],[67,6,67,7],[68,1,68,2],[68,6,68,7],[69,1,69,2],[69,6,69,7],[70,1,70,2],[70,6,70,7],[71,1,71,2],[71,6,71,7],[72,1,72,2],[72,6,72,7],[73,1,73,2],[73,6,73,7],[74,1,74,2],[74,6,74,7],[75,1,75,2],[75,6,75,7],[76,1,76,2],[76,6,76,7],[77,1,77,2],[77,6,77,7],[78,1,78,2],[78,6,78,7],[79,1,79,2],[79,6,79,7],[80,1,80,2],[80,6,80,7],[81,1,81,2],[81,3,81,4],[81,6,81,7],[82,1,82,2],[82,6,82,7],[83,1,83,2],[83,3,83,4],[83,6,83,7],[84,1,84,2],[84,6,84,7],[85,1,85,2],[85,6,85,7],[86,1,86,2],[86,6,86,7],[87,1,87,2],[87,6,87,7],[88,1,88,2],[88,6,88,7],[89,1,89,2],[89,6,89,7],[90,0,90,8],[90,9,90,10]],"flags":["formulas_cached_only"]}
["2019年“D”项目绿化、园建工程量清单与报价表","","","","","","","","","",""]
["工程名称：","","2019年“D”项目绿化、园建工程","","","","",null,"","",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","全费用单价限价(元)","金额（元）"]
["","","","","","","","",null,"全费用单价","合  计"]
[" "," ",null,"一、土方工程 ",null," "," ",null," ",null,""]
["1","050101010001",null,"整理绿化用地","1.场内土方平衡；\r\n2.找平找坡要求：满足设计和施工要求；\r\n3.需起坡造型部位不计算整理绿地工程量。\r\n","m2","5050",null,"3.26",null,""]
["2","050101009054",null,"绿地起坡造型","1.取土运距 ：场内土方平衡，运距投标人综合考虑；\r\n3.起坡平均高度：综合，根据甲方现场要求。","m3","10000",null,"7.66",null,""]
["3","040101001055",null,"挖便道土石方（场地回填）","1.土壤类别：综合考虑\r\n2.挖土石深度：深度综合考虑\r\n3.根据甲方要求施工便道需分段施工（分段栽植苗木，分段拆除便道），土石方场内回填。\r\n4.满足设计及其他规范要求","m3","5000",null,"8.83",null,""]
["4","040101001055",null,"挖便道土石方（外运）","1.土壤类别：综合考虑\r\n2.挖土石方深度：深度综合考虑\r\n3.根据甲方要求施工便道需分段施工（分段栽植苗木，分段拆除便道）\r\n4.外运距离：挖除便道后的土方投标人自行考虑弃土场\r\n5.满足设计及甲方要求","m3","10000",null,"19.67",null,""]
[" "," ",null,"二、乔木 ",null," "," ",null," ",null,""]
["5","050102001001",null,"栽植羊蹄甲 胸径13cm","1.乔木种类：羊蹄甲；\r\n2.乔木规格及要求：胸径13cm，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范；\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","5",null,"212.41",null,""]
["6","050102001003",null,"栽植香樟 胸径11cm","1.乔木种类：香樟；\r\n2.乔木规格及要求：胸径11cm，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范；\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","17",null,"153.85",null,""]
["7","050102001005",null,"栽植小叶榕 胸径10cm","1.乔木种类：小叶榕；\r\n2.乔木规格及要求：胸径10cm，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","16",null,"138.44",null,""]
["8","050102001006",null,"栽植蓝花楹 胸径15cm","1.乔木种类：蓝花楹；\r\n2.乔木规格及要求：胸径15cm，不得随意修剪\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","6",null,"212.41",null,""]
["9","050102006001",null,"栽植桂花 胸径10cm","1.苗木种类：桂花；\r\n2.苗木规格及要求：胸径10cm ，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","2",null,"138.44",null,""]
["10","050102001010",null,"栽植柑橘","1.乔木种类：柑橘 ；\r\n2.乔木规格及要求：地径7cm ，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","20",null,"53.30",null,""]
["11","050102001011",null,"栽植朴树A 胸径19cm","1.乔木种类：朴树A；\r\n2.乔木规格及要求：胸径19cm，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","1",null,"407.08",null,""]
["12","050102001012",null,"栽植朴树B 胸径13cm","1.乔木种类：朴树B；\r\n2.乔木规格及要求：胸径13cm，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","6",null,"222.61",null,""]
["13","050102001016",null,"栽植枫香 胸径11cm","1.乔木种类：枫香；\r\n2.乔木规格及要求：胸径11cm  高度4-5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。\r\n6.支撑: 符合设计及施工规范","株","10",null,"146.26",null,""]
["14","050102001017",null,"栽植乌桕 胸径11cm","1.乔木种类：乌桕 ；\r\n2.乔木规格及要求：胸径11cm 高度4-5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","20",null,"164.05",null,""]
["15","050102001018",null,"栽植皂荚 胸径11cm","1.乔木种类：皂荚；\r\n2.乔木规格及要求：胸径11cm  高度4-5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","21",null,"164.05",null,""]
["16","050102001021",null,"栽植水杉 胸径10cm","1.乔木种类：水杉；\r\n2.乔木规格及要求： 胸径10cm 高6-8m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","9",null,"146.26",null,""]
["17","050102001021",null,"栽植枫杨 胸径10cm","1.乔木种类：枫杨；\r\n2.乔木规格及要求： 胸径10cm  高度4-5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","6",null,"146.26",null,""]
["18","050102001026",null,"栽植垂柳 胸径9cm","1.乔木种类：垂柳；\r\n2.乔木规格及要求：胸径9cm  高度3.5-4m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","23",null,"119.46",null,""]
["19","050102001029",null,"栽植紫玉兰 胸径9cm","1.乔木种类：紫玉兰；\r\n2.乔木规格及要求：胸径9cm  高度3-3.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","5",null,"119.46",null,""]
["20","050102001030",null,"栽植晚樱 地径7-8cm\r\n","1.乔木种类：晚樱；\r\n2.乔木规格及要求：地径7-8cm  高度3-3.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","2",null,"53.30",null,""]
["21","050102001033",null,"栽植红梅 地径6-7cm","1.乔木种类：红梅；\r\n2.乔木规格及要求： 地径6-7cm  高度2-2.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","1",null,"53.30",null,""]
["22","050102001036",null,"栽植紫薇","1.灌木种类：紫薇；\r\n2.灌木规格及要求：地径6cm   高度2-2.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","8",null,"25.60",null,""]
["23","050102001038",null,"栽植木芙蓉","1.乔木种类：木芙蓉；\r\n2.乔木规格及要求：地径6cm 高度2-2.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","70",null,"61.12",null,""]
["24","050102001039",null,"栽植花石榴","1.乔木种类：花石榴；\r\n2.乔木规格及要求： 冠幅1.5-1.8m 高度2-2.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","12",null,"61.12",null,""]
[" "," ",null,"三、灌木 ",null," "," ",null," ",null,""]
["25","050102006003",null,"石楠","1.苗木种类：石楠；\r\n2.苗木规格及要求： 地径8cm ，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.支撑: 符合设计及施工规范\r\n6.做法：满足设计及现行技术、质量、施工验收规范要求。","株","3",null,"41.51",null,""]
["26","050102006006",null,"栽植三角梅球","1.植物种类：三角梅球\r\n2.高度： 高度100-120cm，冠幅100-150cm\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","28",null,"14.05",null,""]
["27","050102001037",null,"栽植木绣球","1.灌木种类：木绣球；\r\n2.灌木规格及要求： 冠幅2-2.5m 高度2-2.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","3",null,"41.51",null,""]
["28","050102002002",null,"栽植紫荆","1.灌木种类：紫荆；\r\n2.灌木规格及要求：冠幅1.5-1.8m 高度2-2.5m，不得随意修剪；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","25",null,"25.60",null,""]
[" "," ",null,"地被植物 ",null," "," ",null," ",null,""]
["29","050102006004",null,"栽植夹竹桃","1.苗木种类：夹竹桃；\r\n2.苗木规格及要求： 冠幅0.2-0.3m 高度0.5-0.6m，9株/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","695",null,"18.53",null,""]
["30","050102007001",null,"栽植春羽","1.植物种类：春羽；\r\n2.植物规格及要求：高度0.6m-0.8m，冠幅0.4m，16株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","59",null,"18.55",null,""]
["31","050102008001",null,"栽植姜花","1.灌木种类：姜花；\r\n2.灌木规格及要求：高度0.4-0.5m  冠幅0.35m，25株/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","268",null,"18.55",null,""]
["32","050102007002",null,"栽植艳山姜","1.植物种类：艳山姜；\r\n2.植物规格及要求：高度0.6m-0.8m，冠幅0.4m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","56",null,"18.55",null,""]
["33","050102007003",null,"栽植醉鱼草","1.植物种类：醉鱼草；\r\n2.植物规格及要求：高度0.6m-0.8m，冠幅0.4m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","48",null,"18.55",null,""]
["34","050102007005",null,"栽植大花美人蕉","1.植物种类：大花美人蕉；\r\n2.植物规格及要求：高度0.6m-0.8m，冠幅0.35m，16株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","66",null,"18.55",null,""]
["35","050102007006",null,"栽植水生美人蕉","1.灌木种类：水生美人蕉；\r\n2.灌木规格及要求： 高度0.6-0.8m 冠幅0.4m ，16株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","215",null,"18.55",null,""]
["36","050102007007",null,"栽植紫茉莉","1.灌木种类：紫茉莉；\r\n2.灌木规格及要求：高度0.3-0.4m 冠幅0.25m，25株/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","215",null,"18.55",null,""]
["37","050102007008",null,"栽植小叶栀子","1.植物种类：小叶栀子；\r\n2.植物规格及要求：高度0.2m-0.25m，冠幅0.25m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","26",null,"18.53",null,""]
["38","050102007009",null,"栽植大花萱草","1.植物种类：大花萱草；\r\n2.植物规格及要求：高度0.3m-0.4m，冠幅0.25m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","118",null,"18.55",null,""]
["39","050102007013",null,"栽植蜘蛛兰","1.植物种类：蜘蛛兰；\r\n2.植物规格及要求：高度0.3m-0.4m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","67",null,"18.55",null,""]
["40","050102007014",null,"栽植冷水花","1.植物种类：冷水花；\r\n2.植物规格及要求：高度0.15m-0.2m，冠幅0.2m，36株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","19",null,"18.55",null,""]
["41","050102007015",null,"栽植活血丹","1.植物种类：活血丹；\r\n2.植物规格及要求：高度0.15m-0.2m，冠幅0.2m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","291",null,"18.55",null,""]
["42","050102007016",null,"栽植毛鹃","1.植物种类：毛鹃；\r\n2.植物规格及要求：高度0.2m-0.25m，冠幅0.25m，25株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","69",null,"18.53",null,""]
["43","050102007021",null,"栽植红花酢浆草","1.灌木种类：红花酢浆草；\r\n2.灌木规格及要求：高度0.15-0.2m 冠幅0.2m，36株/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","380",null,"18.55",null,""]
["44","050102007022",null,"栽植葱兰","1.植物种类：葱兰；\r\n2.植物规格及要求： 高度0.15m-0.2m，36株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","84",null,"18.55",null,""]
["45","050102007022",null,"栽植肾蕨","1.植物种类：肾蕨；\r\n2.植物规格及要求： 高度0.15m-0.2m，36株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","27",null,"25.77",null,""]
["46","050102007024",null,"栽植玉簪","1.植物种类：玉簪；\r\n2.植物规格及要求： 高度0.25m-0.3m， 冠幅0.25m，36株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","75",null,"18.55",null,""]
["47","050102007025",null,"栽植兰花三七","1.植物种类：兰花三七；\r\n2.植物规格及要求： 高度0.15m-0.2m，36株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","181",null,"18.55",null,""]
["48","050102007028",null,"栽植白三叶","1.灌木种类：白三叶；\r\n2.灌木规格及要求：高度0.15-0.2m 36丛/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","438",null,"18.55",null,""]
["49","050102007029",null,"栽植鸢尾","1.植物种类：鸢尾；\r\n2.植物规格及要求：高度0.2m-0.2m，36株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","95",null,"18.55",null,""]
["50","050102007031",null,"栽植蒲苇","1.植物种类：蒲苇；\r\n2.植物规格及要求：高度0.8m-1m，1丛/㎡，20-30芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","542",null,"18.55",null,""]
["51","050102007036",null,"栽植狼尾草","1.植物种类：狼尾草；\r\n2.植物规格及要求：高度0.6m-0.8m，9丛/㎡，10-20芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","105",null,"18.55",null,""]
["52","050102007037",null,"栽植细叶芒","1.植物种类：细叶芒；\r\n2.植物规格及要求：高度0.6m-0.8m，杆数＞3杆，9丛/㎡，10-20芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","184",null,"18.55",null,""]
["53","050102007044",null,"栽植玉带草","1.植物种类：玉带草；\r\n2.植物规格及要求：16丛/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","54",null,"18.55",null,""]
["54","050102007045",null,"栽植金钱蒲","1.植物种类：金钱蒲；\r\n2.植物规格及要求：16丛/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","100",null,"18.55",null,""]
["55","050102007047",null,"栽植玉蝉花","1.植物种类：玉蝉花；\r\n2.植物规格及要求：高度0.5m-1m，16株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","180",null,"25.77",null,""]
["56","050102007035",null,"栽植海芋","1.植物种类：海芋；\r\n2.植物规格及要求：高度0.4-0.5m 冠幅0.4m,16株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","456",null,"25.77",null,""]
["57","050102007052",null,"栽植籽播蛇梅","1.植物种类：蛇梅\r\n2.植物规格及要求：高度0.2m以上，蓬径0.2m以上，杆数＞3杆，100株/㎡，满植；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","391",null,"11.87",null,""]
["58","050102007032",null,"栽植芦竹","1.植物种类：芦竹；\r\n2.植物规格及要求：高度0.8m-1.2m，9丛/㎡，4-5芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","454",null,"1.33",null,""]
["59","050102007030",null,"栽植水葱","1.植物种类：水葱；\r\n2.植物规格及要求：高度0.8m-1m，25丛/㎡，15-20芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","1050",null,"1.99",null,""]
["60","050102007033",null,"栽植芦苇","1.植物种类：芦苇；\r\n2.植物规格及要求：高度0.8-1.2m，5丛/m2,10芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","2500",null,"1.66",null,""]
["61","050102007041",null,"栽植香蒲","1.植物种类：香蒲；\r\n2.植物规格及要求：高度0.3m-0.6m，16株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","296",null,"1.33",null,""]
["62","050102007046",null,"栽植黄菖蒲","1.植物种类：黄菖蒲；\r\n2.植物规格及要求：高度0.5m-1m，16丛/㎡，2-3芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","4160",null,"1.33",null,""]
["63","050102007039",null,"栽植慈姑","1.植物种类：慈姑；\r\n2.植物规格及要求：高度0.3m-0.5m，9株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","1728",null,"1.33",null,""]
["64","050102009002",null,"栽植旱伞草","1.植物种类：旱伞草；\r\n2.植物规格及要求：高度0.6m-0.8m，9丛/㎡，20-30芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","423",null,"1.99",null,""]
["65","050102007042",null,"栽植野茭白","1.植物种类：野茭白；\r\n2.植物规格及要求：高度0.3m-0.6m，16株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","10048",null,"1.33",null,""]
["66","050102007034",null,"栽植再力花","1.植物种类：再力花；\r\n2.植物规格及要求：高度0.7m-0.8m，5丛/m2,10芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","2160",null,"1.11",null,""]
["67","050102009001",null,"栽植千屈菜","1.植物种类：千屈菜；\r\n2.植物规格及要求：高度0.7m-0.8m，9株/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","3132",null,"1.11",null,""]
["68","050102007043",null,"栽植梭鱼草","1.植物种类：梭鱼草；\r\n2.植物规格及要求：高度0.2m-0.3m，9丛/㎡，3-4芽/丛；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","168",null,"0.66",null,""]
["69","050102007040",null,"栽植水芹","1.植物种类：水芹；\r\n2.植物规格及要求：高度0.3m-0.5m，16丛/㎡；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","丛","2624",null,"0.66",null,""]
["70","050102009003",null,"栽植菱","1.植物种类：菱；\r\n2.植物规格及要求：4缸/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","564",null,"1.49",null,""]
["71","050102007048",null,"栽植蓬萍草","1.植物种类：蓬萍草；\r\n2.植物规格及要求：胸径0.15-0.2m，2缸/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","200",null,"1.49",null,""]
["72","050102009004",null,"栽植荷花","1.植物种类：荷花；\r\n2.植物规格及要求：2缸/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","1748",null,"2.13",null,""]
["73","050102009005",null,"栽植睡莲","1.植物种类：睡莲；\r\n2.植物规格及要求：2缸/m2；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","缸","516",null,"2.13",null,""]
[" "," ",null,"驳岸做法一 ",null," "," ",null," ",null,""]
["74","050202001001",null,"石（卵石）砌驳岸一","1.石料种类、规格：点缀景石 (材料甲供)\r\n2.驳岸截面、长度 ：详设计施工图\r\n3.场内运输：投标人自行考虑；\r\n4.做法：满足设计施工图及现行技术、质量验收规范要求","t","500",null,"234.78",null,""]
[" "," ",null,"驳岸做法四 ",null," "," ",null," ",null,""]
["75","010101002003",null,"挖一般土方","1.土壤类别：综合\r\n2.挖土深度：综合\r\n3.用于场内平衡，运距投标人综合考虑\r\n4.满足设计及其他规范要求","m3","2033.76",null,"8.61",null,""]
["76","010103001003",null,"基础土石方回填","1.填方材料品种：满足设计和施工验收规范要求\r\n2.密实度：按设计和施工验收规范要求\r\n3.回填土来源及场内外运输方式、运距：投标人自行考虑\r\n4.回填部位：详见设计。\r\n5.做法：回填土应满足设计及现行施工技术、质量验收规范要求","m3","1635.168",null,"5.29",null,""]
["77","010103002002",null,"余方弃置","1.废弃料品种：综合\r\n2.弃土、石场费用及场内外运距：投标人自行综合考虑\r\n3.做法：满足设计及现行施工技术、质量验收规范要求","m3","380.592",null,"6.74",null,""]
["78","010501001031",null,"100厚C20素混凝土垫层","1.工程内容：100mm厚C20砼垫层\r\n2.混凝土强度等级：C20商品砼\r\n3.厚度：100mm\r\n4.砼运输及泵送方式：由投标人综合考虑\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","m3","55.36",null,"498.85",null,""]
["79","010403001004",null,"MU20毛石基础","1.石料种类、规格：MU20毛石\r\n2.石表面加工及勾缝要求：详设计施工图   \r\n3.场内运输：投标人自行考虑；\r\n4.砂浆强度等级、配合比：水泥砂浆(特细砂) M10\r\n5、满足设计及其他规范要求","m3","343.232",null,"350.43",null,""]
["80","050202003054",null,"满(散)铺砂卵石护岸   （自然护岸）","1.护岸平均宽度 \r\n2.粗细砂比例 \r\n3.卵石粒径","m2","535.6",null,"165.86"]
["合　　计（大写：                                                  ）","","","","","","","","",null,""]