{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["【园林绿化工程】"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"【园林绿化工程】","index":0,"n_rows":59,"n_cols":11,"rows_kept":59,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,6],[1,7,1,8],[1,9,1,10],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,7],[2,8,3,8],[2,9,2,10],[4,1,4,2],[4,6,4,7],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,1,13,2],[13,6,13,7],[14,1,14,2],[14,6,14,7],[15,1,15,2],[15,6,15,7],[16,1,16,2],[16,6,16,7],[17,1,17,2],[17,6,17,7],[18,1,18,2],[18,6,18,7],[19,1,19,2],[19,6,19,7],[20,1,20,2],[20,6,20,7],[21,1,21,2],[21,6,21,7],[22,1,22,2],[22,6,22,7],[23,1,23,2],[23,6,23,7],[24,1,24,2],[24,6,24,7],[25,1,25,2],[25,6,25,7],[26,1,26,2],[26,6,26,7],[27,1,27,2],[27,6,27,7],[28,1,28,2],[28,6,28,7],[29,1,29,2],[29,6,29,7],[30,1,30,2],[30,6,30,7],[31,1,31,2],[31,6,31,7],[32,1,32,2],[32,6,32,7],[33,1,33,2],[33,6,33,7],[34,1,34,2],[34,6,34,7],[35,1,35,2],[35,6,35,7],[36,1,36,2],[36,6,36,7],[37,1,37,2],[37,6,37,7],[38,1,38,2],[38,6,38,7],[39,1,39,2],[39,6,39,7],[40,1,40,2],[40,6,40,7],[41,1,41,2],[41,6,41,7],[42,1,42,2],[42,6,42,7],[43,1,43,2],[43,6,43,7],[44,1,44,2],[44,6,44,7],[45,1,45,2],[45,6,45,7],[46,1,46,2],[46,6,46,7],[47,1,47,2],[47,6,47,7],[48,1,48,2],[48,6,48,7],[49,1,49,2],[49,6,49,7],[50,1,50,2],[50,6,50,7],[51,1,51,2],[51,6,51,7],[52,1,52,2],[52,6,52,7],[53,1,53,2],[53,6,53,7],[54,1,54,2],[54,6,54,7],[55,1,55,2],[55,6,55,7],[56,1,56,2],[56,6,56,7],[57,1,57,2],[57,6,57,7],[58,0,58,8],[58,9,58,10]],"flags":["formulas_cached_only"]}
["2019年“I”项目绿化种植工程量清单与报价表","","","","","","","","","",""]
["工程名称：","","2019年“I”项目绿化种植工程","","","","",null,"","",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","全费用单价限价(元)","金额（元）"]
["","","","","","","","",null,"全费用单价","合  计"]
[" "," ","","乔木"," "," "," ",""," ",null,""]
["1","050102001001","","栽植香樟：米径30cm，高7-8米，冠3.5-4m","1.乔木种类：栽植香樟（甲供材）\r\n2.土球及乔木规格：米径30cm，高7-8米，冠3.5-4m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","5","","745.28",null,""]
["2","050102001001","","栽植香樟：米径18cm，高6-7米，冠2.5-3m","1.乔木种类：栽植香樟（甲供材）\r\n2.土球及乔木规格：米径18cm，高6-7米，冠2.5-3m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","23","","443.82",null,""]
["3","050102001001","","栽植皂角：米径25cm，高6-7米，冠4-4.5m","1.乔木种类：栽植皂角（甲供材）\r\n2.土球及乔木规格：米径25cm，高6-7米，冠4-4.5m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","5","","636.42",null,""]
["4","050102001001","","栽植朴树：米径25cm，高6-7米，冠4-4.5m","1.乔木种类：栽植朴树（甲供材）\r\n2.土球及乔木规格：米径25cm，高6-7米，冠4-4.5m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","9","","647.54",null,""]
["5","050102001001","","栽植银杏：米径30cm，高7-8米，冠3.5-4m","1.乔木种类：栽植银杏（甲供材）\r\n2.土球及乔木规格：米径30cm，高7-8米，冠3.5-4m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","19","","745.28",null,""]
["6","050102001001","","栽植蓝花楹：米径18cm，高5.5-6米，冠4-4.5米","1.乔木种类：栽植蓝花楹（甲供材）\r\n2.土球及乔木规格：米径18cm，高5.5-6米，冠4-4.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","26","","443.82",null,""]
["7","050102001001","","栽植蓝花楹：米径12cm，高3.5-6米，冠4-4.5米","1.乔木种类：栽植蓝花楹（甲供材）\r\n2.土球及乔木规格：米径12cm，高3.5-6米，冠4-4.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","105","","154.07",null,""]
["8","050102001001","","栽植蓝花楹：米径7-8cm，高2.5-3米，冠2.5-3米","1.乔木种类：栽植蓝花楹（甲供材）\r\n2.土球及乔木规格：米径7-8cm，高2.5-3米，冠2.5-3米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","33","","83.81",null,""]
["9","050102001001","","栽植小叶榕：米径30cm，高6-7米，冠3.5-4m","1.乔木种类：栽植小叶榕（甲供材）\r\n2.土球及乔木规格：米径30cm，高6-7米，冠3.5-4m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","8","","745.28",null,""]
["10","050102001001","","栽植柳树：米径15cm，高5-5.5米，冠3-3.5m","1.乔木种类：栽植柳树（甲供材）\r\n2.土球及乔木规格：米径15cm，高5-5.5米，冠3-3.5m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","24","","278.19",null,""]
["11","050102001001","","栽植紫玉兰：米径8cm，高3-3.5米，冠2.5-3m","1.乔木种类：栽植紫玉兰（甲供材）\r\n2.土球及乔木规格：米径8cm，高3-3.5米，冠2.5-3m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","15","","90.91",null,""]
["12","050102001001","","栽植白玉兰：米径8cm，高3-3.5米，冠2.5-3m","1.乔木种类：栽植白玉兰（甲供材）\r\n2.土球及乔木规格：米径8cm，高3-3.5米，冠2.5-3m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","11","","90.91",null,""]
["13","050102001001","","栽植红花羊蹄甲：米径12cm，高3-3.5米，冠2-2.5米","1.乔木种类：栽植红花羊蹄甲（甲供材）\r\n2.土球及乔木规格：米径12cm，高3-3.5米，冠2-2.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","7","","149.89",null,""]
["14","050102001001","","栽植红梅：地径6cm，高2.5-3米，冠2.5-3米","1.乔木种类：栽植红梅（甲供材）\r\n2.土球及乔木规格：地径6cm，高2.5-3米，冠2.5-3米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","43","","43.87",null,""]
["15","050102001001","","栽植丛生紫薇：地径10cm，高2-2.5米，冠2-2.5米","1.乔木种类：栽植丛生紫薇（甲供材）\r\n2.土球及乔木规格：地径10cm，高2-2.5米，冠2-2.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","45","","108.05",null,""]
["16","050102001001","","栽植桂花：米径10cm，高3-3.5米，冠2.5-3m","1.乔木种类：栽植桂花（甲供材）\r\n2.土球及乔木规格：米径10cm，高3-3.5米，冠2.5-3m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","28","","126.60",null,""]
["17","050102001001","","栽植红叶李：米径12-15cm，高3-3.5米，冠2.5-3m","1.乔木种类：栽植红叶李（甲供材）\r\n2.土球及乔木规格：米径12-15cm，高3-3.5米，冠2.5-3m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","12","","149.89",null,""]
["18","050102001001","","栽植碧桃：地径6cm，高2.5-3米，冠2.5-3米","1.乔木种类：栽植碧桃（甲供材）\r\n2.土球及乔木规格：地径6cm，高2.5-3米，冠2.5-3米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","67","","43.87",null,""]
["19","050102001001","","栽植垂丝海棠：米径8cm，高3-3.5米，冠2.5-3m","1.乔木种类：栽植垂丝海棠（甲供材）\r\n2.土球及乔木规格：米径8cm，高3-3.5米，冠2.5-3m，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","45","","83.81",null,""]
["20","050102001001","","栽植红枫：地径6cm，高2-2.5米，冠1.5-2米","1.乔木种类：栽植红枫（甲供材）\r\n2.土球及乔木规格：地径6cm，高2-2.5米，冠1.5-2米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","25","","48.97",null,""]
["21","050102001001","","栽植罗汉松桩景：地径15-16cm，高2.5-3米，冠2-2.5米","1.乔木种类：栽植罗汉松桩景（甲供材）\r\n2.土球及乔木规格：地径15-16cm，高2.5-3米，冠2-2.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","1","","165.03",null,""]
["22","050102001001","","栽植罗汉松桩景：地径10-12cm，高1.8-2米，冠1.5-1.8米","1.乔木种类：栽植罗汉松桩景（甲供材）\r\n2.土球及乔木规格：地径10-12cm，高1.8-2米，冠1.5-1.8米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","1","","108.05",null,""]
["23","050102001001","","栽植罗汉松桩景：地径8-10cm，高1.2-1.5米，冠1-1.2米","1.乔木种类：栽植罗汉松桩景（甲供材）\r\n2.土球及乔木规格：地径8-10cm，高1.2-1.5米，冠1-1.2米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","1","","108.05",null,""]
["24","050102001001","","栽植榕树桩景：地径35-40cm，高2-2.5米，冠1.8-2米","1.乔木种类：栽植榕树桩景（甲供材）\r\n2.土球及乔木规格：地径35-40cm，高2-2.5米，冠1.8-2米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","1","","643.41",null,""]
["25","050102001001","","栽植榕树桩景：地径25-30cm，高1.2-1.5米，冠1.5-1.8米","1.乔木种类：栽植榕树桩景（甲供材）\r\n2.土球及乔木规格：地径25-30cm，高1.2-1.5米，冠1.5-1.8米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","1","","538.89",null,""]
["26","050102001001","","栽植地笼桂花：高2.5-2.8米，冠2-2.5米","1.乔木种类：栽植地笼桂花（甲供材）\r\n2.土球及乔木规格：高2.5-2.8米，冠2-2.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","36","","108.05",null,""]
["27","050102001001","","栽植红叶石楠球：高1.2米，冠1.2-1.5米","1.乔木种类：栽植红叶石楠球（甲供材）\r\n2.土球及乔木规格：高1.2米，冠1.2-1.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","108","","24.03",null,""]
["28","050102001001","","栽植红继木球：高1.2米，冠1.2-1.5米","1.乔木种类：栽植红继木球（甲供材）\r\n2.土球及乔木规格：高1.2米，冠1.2-1.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","68","","24.03",null,""]
["29","050102001001","","栽植金禾女贞球：高1.2米，冠1.2-1.5米","1.乔木种类：栽植金禾女贞球（甲供材）\r\n2.土球及乔木规格：高1.2米，冠1.2-1.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","82","","24.03",null,""]
["30","050102001001","","栽植杜鹃球：高1.2米，冠1.2-1.5米","1.乔木种类：栽植杜鹃球（甲供材）\r\n2.土球及乔木规格：高1.2米，冠1.2-1.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","44","","24.03",null,""]
["31","050102001001","","栽植海桐球：高1.2米，冠1.2-1.5米","1.乔木种类：栽植海桐球（甲供材）\r\n2.土球及乔木规格：高1.2米，冠1.2-1.5米，不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","67","","24.03",null,""]
["32","050102001001","","栽植紫竹：米径2cm，冠2-2.5米","1.乔木种类：栽植紫竹（甲供材）\r\n2.土球及乔木规格：米径2cm，冠2-2.5米，4株/m不得随意修剪\r\n3.养护：100%成活率；养护期一年 \r\n4.支撑: 符合设计及施工规范\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求","株","896","","36.78",null,""]
["33","050101009002","","种植土回填","1.回填土质要求 ：投标人自行考虑外购\r\n2.取土运距 ：投标人根据现场自行考虑，涉及运种植土到树池等\r\n3.回填厚度 \r\n4.弃土运距","m3","9353.5","","22.78",null,""]
["34","050101010011","","整理绿化用地","1.回填土质要求 \r\n2.取土运距 \r\n3.回填厚度 综合考虑0.5m，实际工程量以现场收方为准\r\n4.找平找坡要求 \r\n5.弃渣运距","m2","18709","","3.94",null,""]
[" "," ","","绿化工程"," "," "," ",""," ",null,""]
["35","050102007035","","栽植西洋鹃","1.植物种类：西洋鹃（甲供材）；\r\n2.植物规格及要求：高度0.2m 冠幅0.2m,64株/m2，生长良好；\r\n3.场内运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","713","","18.75",null,""]
["36","050102007035","","栽植木春菊","1.植物种类：木春菊（甲供材）；\r\n2.植物规格及要求：高度0.25m 冠幅0.2m,49株/m2，生长良好；\r\n3.场内运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","484","","18.75",null,""]
["37","050102007035","","栽植翠芦莉","1.植物种类：翠芦莉（甲供材）；\r\n2.植物规格及要求：高度0.25m 冠幅0.2m,49株/m2，生长良好；\r\n3.场内运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","664","","18.75",null,""]
["38","050102007035","","栽植金禾女贞","1.植物种类：金禾女贞（甲供材）；\r\n2.植物规格及要求：高度0.25m 冠幅0.2m,49株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","548","","18.75",null,""]
["39","050102007035","","栽植红继木","1.植物种类：红继木（甲供材）；\r\n2.植物规格及要求：高度0.25m 冠幅0.2m,64株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","194","","18.75",null,""]
["40","050102007035","","栽植红叶石楠","1.植物种类：红叶石楠（甲供材）；\r\n2.植物规格及要求：高度0.25m 冠幅0.2m,49株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","716","","18.75",null,""]
["41","050102007035","","栽植冷水花","1.植物种类：冷水花（甲供材）；\r\n2.植物规格及要求：高度0.2m 冠幅0.2m,49株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","30","","18.75",null,""]
["42","050102007035","","栽植肾蕨","1.植物种类：肾蕨（甲供材）；\r\n2.植物规格及要求：高度0.3m 冠幅0.2m,49株/m2，生长良好；\r\n3.场内运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","271","","18.75",null,""]
["43","050102007035","","栽植西伯利亚鸢尾","1.植物种类：西伯利亚鸢尾（甲供材）；\r\n2.植物规格及要求：高度0.5m 冠幅0.2m,36株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","227","","18.75",null,""]
["44","050102007035","","栽植再力花","1.植物种类：再力花（甲供材）；\r\n2.植物规格及要求：高度1m 冠幅0.4m,36株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","190","","18.75",null,""]
["45","050102007035","","栽植旱伞草","1.植物种类：旱伞草（甲供材）；\r\n2.植物规格及要求：高度1m 冠幅0.3m,5-8株/丛，16丛/m2，生长良好；\r\n3.场内运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","110","","18.75",null,""]
["46","050102007035","","栽植水生美人蕉","1.植物种类：海芋（甲供材）；\r\n2.植物规格及要求：高度0.8m 冠幅0.3m,25株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","146","","18.75",null,""]
["47","050102007035","","栽植梭鱼草","1.植物种类：梭鱼草（甲供材）；\r\n2.植物规格及要求：高度0.8m 冠幅0.3m,36株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","123","","18.75",null,""]
["48","050102007035","","栽植时令鲜花 一年共六次","1.植物种类：栽植时令鲜花（甲供材）；一年换6次\r\n2.植物规格及要求：高度0.2m 冠幅0.2m,100株/m2，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m2","593","","75.99",null,""]
["49","050102009004","","栽植太空荷花","1.植物种类：荷花；\r\n2.植物规格及要求；\r\n3.场内运输：投标人自行考虑；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","株","300","","1.55",null,""]
["50","050102012008","","台湾二号草坪","1.草皮种类  台湾二号\r\n2.铺种方式 满铺\r\n3.养护期12个月","m2","13700","","21.37",null,""]
["51","050102008004","","栽植三角梅（藤长1.2m-1.5m）","1.花卉种类 ：栽植三角梅\r\n2、株高或蓬径 ：（藤长1.2m-1.5m）\r\n3.养护期：12个月，包成活","株","1100","","9.80",null,""]
["52","050102005036","","栽植冬青","1.植物种类：冬青（甲供材）；\r\n2.植物规格及要求：高度1.5-1.8m 冠幅0.3m,6株/m，生长良好；\r\n3.场内外运输方式及运输距离：承包人自定；\r\n4.养护及养护期：100%成活率；养护期12个月；\r\n5.做法：满足设计及现行技术、质量、施工验收规范要求。","m","198","","25.70",null,""]
["合　　计（大写：                                                  ）","","","","","","","","",null,""]