{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["小品1","WpsReserved_CellImgList"],"not_rendered":{"images":8,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"小品1","index":0,"n_rows":14,"n_cols":9,"rows_kept":14,"merged":[[0,0,0,8],[9,0,9,5],[9,6,9,8],[10,0,10,8],[11,4,11,7],[12,4,12,7],[13,4,13,7]]}
["2023年“S”项目景观雕塑小品采购报价表（a）"]
["序号","项目名称","规格材质","单位","数量","全费用单价限价（元）","班组所报单价（元）","合价（元）","备注"]
[1,"定制成品坐凳","1.材质:镀锌板+菠萝格木\n2.尺寸：长150cm*宽50cm*高76cm\n3.安装固定方式由投标人自行考虑","个",135,1200]
[2,"垃圾投放点","1.成品，材质为镀锌板，尺寸2.4mX0.8mX2m\n2.安装固定方式由投标人自行考虑","个",1,7000]
[3,"成品三分类垃圾桶","1.成品，材质为镀锌板，尺寸1.08mX0.4mX0.96m\n2.安装固定方式由投标人自行考虑","个",66,650]
[4,"成品桌椅组合（一桌四椅）","1.材质:铝合金框架、塑木桌子\n2.尺寸:直径80*74高\n3.座椅尺寸:55*55*86cm\n4.桌子底部固定桌椅有效链接\n5.安装固定方式由投标人自行考虑","套",37,1200]
[5,"成品隔离墩","1.成品，清水混凝土材质为主，顶部为不锈钢，间隔1.5米布置\n2.安装固定方式由投标人自行考虑","个",28,250]
[6,"自行车停车架","1.成品，材质为镀锌板，壁厚不小于5mm,底板不小于1cm 灰色烤漆，丝印图案，采用膨胀螺栓固定长度不低于10cm,间隔0.5m按图布置。\n2.安装固定方式由投标人自行考虑","个",71,200]
[7,"减速带","1.成品，铸铁材质，宽280mm，高45mm，采用膨胀螺栓固定，按图安装。","m",{"$f":"6*4+5.7+6","v":35.7},150]
["合  计                            金额：                    元 ",{"$nulls":5},"开具发票税率：         %"]
["注：1.本次采用全费用单价报价形式，最高限价为282855.00元，施工单位所报价高于最高限价的为无效报价，采购人不予接受。同时在工程量清单中公布最高费用单价限价，施工单位的全费用单价限价，施工单位的全费用单价也不得超过最高全费用单价限价，否则，采购人将予以拒绝。\n2.最终结算时，以经审计单位核定的实际完成工程量及有效的竣工资料进行计算，全费用单价按中选的全费用单价进行计价。\n3.供应商应具备雕塑、小品二次深化设计能力，中选单位须于中选后3天内完成符合业主方要求的二次深化设计并提交业主方审核。\n4.开具的发票为增值税专票（13%或9%税率或6%税率或3%或1%税率）。"]
[{"$nulls":4},"报价单位：（盖章）"]
[{"$nulls":4},"委托代理人及电话："]
[{"$nulls":4},"时间："]

{"sheet":"WpsReserved_CellImgList","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}